this code should run fine in most ESP dev boards with an 'RFID-RC522' chip (i got mine from aliexpress xd) - display support will be added at some point

this has to be run with 'sasa-membership' as its server

USE HTTP INSTEAD OF HTTPS FOR REPORTS. https adds just over a second of delay to the already not 'amazingly fast' system lol
